**DC5V 4020 Hydraulic Centrifugal Fan with XH2.54-2P 30CM Cable**



**Specification**

Voltage: DC 5V

Rated current: 0.19A

Size: 40\*40\*20MM

Power consumption: 0.95W

Speed: 6000±5%RPM

Noise: 25.3DBA

Weight: 22.6g

Lifespan: 28000 hours 40℃


Bearing structure: hydraulic bearing


Wiring: red wire positive, black wire negative

Temperature range: -10 to +60℃

Storage Humidity: 5 to 95%RH

**Dimensional drawings**

****

****