

****Module main parameters:****

****Input voltage****：9~12V

****Max load current****：1.3A

****Receiving output voltage current****：5V/2A,12V/700mA

****Launch coil size: outside diameter 43mm, thickness 2.3mm****

****Launch module size: 18mm\*8.5mm\*15mm****

****Receiving module size: 10mm\*25mm\*3mm****

****Receiving coil size: outside diameter 43mm, thickness 1.2mm****

****Receiving the best distance: 3~6mm****